




Allow mac address 70a5 only, if you plugin other mac address all the witch port will shutdown, including below image (all ports get shutdown)


Its call psecure-violation error









Generate crypto for the switch router:





Hex decimal







File hash check:









Check marlicious attack check signature against ids database





Penetration testing and security audit.

Penetration testing is pretend to attack from an external/internal into the network.



32 bits network:

Class a use 8 bit network and 24 bits nodes

Class b is 16bits networks and 16bits nodes

Class c use 24 bits networks and 8 bit node

Create 2 way trust:

